

Please use a Windows computer to upgrade the firmware.

1. Open the corresponding folder, then extract the file: A8387\_FW&TOOL\_20240815094222.zip




2. After unzipping, select the corresponding folder and double-click: G-Upgrade




3. Connect the product's PD charging port to the computer's USB Type-C port using a USB Type-C cable. All downstream interfaces on the product have been removed.



4. Click Load to select the BIN file, then choose the USB channel. Click Cur Ver to read the version and verify the channel is properly connected. Proceed with Auto for automatic programming.





5. Programming complete

